**Use of SI Air (SIAC) – notes for competitors.**

These notes are intended for small events run by FVO. At larger events, especially major championships there may be slight variations to the procedure so always read the event details beforehand!

After clearing your SIAC but before starting you need to use a Check unit to activate your SIAC (a faint green light in the tip of the SIAC will flash every 4 seconds).

Do not punch the Start unit until the SIAC has stopped beeping from the check process (otherwise the start will not register).

All controls should be SI Air mode but if for any reason a unit does not respond remember to punch the control.

The Finish will be a punching finish and the finish will turn off your SIAC

Note that SportIdent recommend not using a SIAC on the same arm as a GPS watch.